# 3.3.12 - VLAN Configuration

## Part 1 - Step 2

### What benefits can VLANs provide to the network?

To separate sensitive data on different networks


## Part 3 - Step 4

### Although the access ports are assigned to the appropried VLANs, were the pings successful? Explain

No, because there is a phone between S3 and PC4, which is on the VLAN 150.
